| Area | Max Freq | Min Latency | Power | Energy | EDAP |
| --- | --- | --- | --- | --- | --- |
| 4.59353e-3(mm^2) | 1.3175 GHz | 2277 ns | 9.2 mW | 20950 pJ | 219125.85 |

Area and Power reported by primetime

Max Freq at clk = 759

Min Latency assumes 3 cycles ?

Energy = Power \* Min Latency